**MANUFACTURER CALIBRATION REPORT**

|  |  |  |
| --- | --- | --- |
|  | MAIN INFORMATIONS | |
| 1 | Racing Class : | FIA CROSS CAR |
| 2 | Manufacture : |  |
| 3 | Bike Model and Year : |  |
| 4 | Engine Specs : | YAMAHA R6 2012 |
| 5 | Release Date : |  |
| 6 | Approved Manufacturer : |  |
| 7 | Approved Mectronik : |  |
| 8 | Approved FIM : |  |
|  | CALIBRATION ID | |
| 9 | Map Name : | R612AE02 |
| 10 | Map Checksum : | 0x68D32887 |
|  | TEST CONDITIONS | |
| 11 | Firmware Version : | 1.18.29 – 1.18.31 |
| 12 | Base Map Name : | R612AE02 |
| 13 | Base Map Checksum : | 0x68D32887 |
| 14 | Air Temperature : |  |
| 15 | Air Pressure : |  |
| 16 | Fuel : |  |
| 17 | Air Filter : |  |
| 18 | Exhaust Pipe : |  |
| 19 | Trumpets : |  |
| 20 | Restrictors: |  |
| 21 | RPM Limit : |  |
| 22 | Drop Off Strategy : |  |
| 23 | Changes to Injection : |  |
| 24 | Changes to Ignition : |  |
| 25 | Other Changes : |  |
| 26 | Notes : |  |
|  |  |  |